# Title 24.1 — State Electrical Board

## Article 24.1-06 — Electrical Wiring Standards

## Chapter 24.1-06-06 — Special Equipment

### § 24.1-06-06-01. [Reserved].

### § 24.1-06-06-02. [Reserved].

### § 24.1-06-06-03. [Reserved].

### § 24.1-06-06-04. [Reserved].

### § 24.1-06-06-05. [Reserved].

### § 24.1-06-06-06. [Reserved].

### § 24.1-06-06-07. [Reserved].

### § 24.1-06-06-08. [Reserved].

### § 24.1-06-06-09. [Reserved].

### § 24.1-06-06-10. [Reserved].


### § 24.1-06-06-11. [Reserved].

### § 24.1-06-06-12. [Reserved].

### § 24.1-06-06-13. [Reserved].

### § 24.1-06-06-14. [Reserved].

### § 24.1-06-06-15. [Reserved].

### § 24.1-06-06-16. [Reserved].

### § 24.1-06-06-17. [Reserved].

### § 24.1-06-06-18. [Reserved].

### § 24.1-06-06-19. [Reserved].

### § 24.1-06-06-20. [Reserved].

### § 24.1-06-06-21. [Reserved].

### § 24.1-06-06-22. [Reserved].

### § 24.1-06-06-23. [Reserved].

### § 24.1-06-06-24. [Reserved].

### § 24.1-06-06-25. (NEC 625) Electric vehicle charging system.

625.41 Overcurrent protection. Overcurrent protection for feeders and branch circuits supplying
vehicle charging equipment must be sized for continuous duty and must have a rating of not less than
one hundred twenty-five percent of the maximum load of the equipment. For these installations,
"maximum load of equipment" means the setting the electrician adjusted the device to. The adjustment
may not be readily accessible or cannot easily be adjusted by the consumer. The electrician shall label
the device if set to a value less than the maximum nameplate rating. The contractor shall assure the
size of the service feeding these devices is adequate.
History: Effective October 1, 2020.
General Authority: NDCC 43-09-05
Law Implemented: NDCC 43-09-21, 43-09-22
