# Title 38 — Highway Patrol

## Article 38-05 — Flagging and Lighting Requirements for Vehicles and Loads Exempt from Width Limitations

## Chapter 38-05-03 — Lighting Requirements

### § 38-05-03-01. Lighting requirements.

All vehicles and loads exempt from width limitations that are authorized to travel between sunset
and sunrise shall meet the lighting requirements as provided for in North Dakota Century Code chapter
39-21. Every vehicle used for towing or hauling an implement of husbandry and every self-propelled
implement of husbandry may, in addition to the lighting requirements, be equipped with a lighted
rotating or flashing amber light or lights that are clearly visible from the front and rear for a minimum
five hundred feet [152.4 meters].
History: Effective June 1, 1986.
General Authority: NDCC 39-12-04
Law Implemented: NDCC 39-12-04
